//Copyright (C)2014-2023 Gowin Semiconductor Corporation.
//All rights reserved.


1. PnR Messages

  <Report Title>: PnR Report
  <Design File>: H:\01_gaoyun\gao_project\60_uart_ddr3_tft_hdmi_sobel_filter\uart_ddr3_tft_hdmi_sobel_filter\impl\gwsynthesis\uart_ddr3_tft_hdmi_sobel_filter.vg
  <Physical Constraints File>: H:\01_gaoyun\gao_project\60_uart_ddr3_tft_hdmi_sobel_filter\uart_ddr3_tft_hdmi_sobel_filter\src\uart_ddr3_tft_hdmi_sobel_filter.cst
  <Timing Constraints File>: ---
  <PnR Version>: V1.9.9 Beta-3
  <Part Number>: GW5A-LV25UG324ES
  <Device>: GW5A-25
  <Device Version>: A
  <Created Time>:Wed Aug 30 14:39:15 2023


2. PnR Details

  Running placement:
    Placement Phase 0: CPU time = 0h 0m 4s, Elapsed time = 0h 0m 4s
    Placement Phase 1: CPU time = 0h 0m 0.515s, Elapsed time = 0h 0m 0.515s
    Placement Phase 2: CPU time = 0h 0m 23s, Elapsed time = 0h 0m 23s
    Placement Phase 3: CPU time = 0h 0m 34s, Elapsed time = 0h 0m 34s
    Total Placement: CPU time = 0h 1m 1s, Elapsed time = 0h 1m 1s
 Running routing:
    Routing Phase 0: CPU time = 0h 0m 0.006s, Elapsed time = 0h 0m 0.005s
    Routing Phase 1: CPU time = 0h 0m 29s, Elapsed time = 0h 0m 29s
    Routing Phase 2: CPU time = 0h 0m 0.219s, Elapsed time = 0h 0m 0.218s
    Routing Phase 3: CPU time = 0h 0m 0s, Elapsed time = 0h 0m 0s
    Total Routing: CPU time = 0h 0m 29s, Elapsed time = 0h 0m 29s
 Generate output files:
    CPU time = 0h 0m 3s, Elapsed time = 0h 0m 3s

 Total Time and Memory Usage: CPU time = 0h 1m 34s, Elapsed time = 0h 1m 34s, Peak memory usage = 527MB


3. Resource Usage Summary

  ----------------------------------------------------------
  Resources                   | Usage
  ----------------------------------------------------------
  Logic                       | 10153/23040  45%
    --LUT,ALU,ROM16           | 10081(9480 LUT, 601 ALU, 0 ROM16)
    --SSRAM(RAM16)            | 12
  Register                    | 12077/23685  51%
    --Logic Register as Latch | 0/23040  0%
    --Logic Register as FF    | 12075/23040  53%
    --I/O Register as Latch   | 0/645  0%
    --I/O Register as FF      | 2/645  <1%
  CLS                         | 10569/11520  92%
  I/O Port                    | 95
  I/O Buf                     | 92
    --Input Buf               | 4
    --Output Buf              | 70
    --Inout Buf               | 18
  IOLOGIC                     | 60%
    --ODDR                    | 8
    --IDES8_MEM               | 16
    --OSER8                   | 24
    --OSER8_MEM               | 20
    --IODELAY                 | 16
  BSRAM                       | 40%
    --SDPB                    | 14
    --SDPX9B                  | 8
  DSP                         | 0%
  PLL                         | 2/6  34%
  DDRDLL                      | 1/4  25%
  DCS                         | 0/8  0%
  DQCE                        | 1/24  5%
  OSC                         | 0/1  0%
  CLKDIV                      | 2/16  13%
  DLLDLY                      | 0/8  0%
  DQS                         | 2/8  25%
  DHCEN                       | 1/16  7%
  ==========================================================



4. I/O Bank Usage Summary

  -----------------------
  I/O Bank  | Usage       
  -----------------------
  bank 0   | 27/30(90%)  
  bank 1   | 26/29(89%)  
  bank 2   | 17/27(62%)  
  bank 3   | 15/27(55%)  
  bank 4   | 1/35(2%)    
  bank 5   | 9/25(36%)   
  bank 6   | 0/17(0%)    
  bank 7   | 0/27(0%)    
  bank 10  | 0/4(0%)     
  =======================


5. Global Clock Usage Summary

  -------------------------------
  Global Clock  | Usage       
  -------------------------------
  PRIMARY       | 6/8(75%)
  LW            | 8/8(100%)
  GCLK_PIN      | 9/20(45%)
  PLL           | 0/6(0%)
  DDRDLL        | 1/4(25%)
  CLKDIV        | 2/16(13%)
  DLLDLY        | 0/8(0%)
  ===============================


6. Global Clock Signals

  -------------------------------------------
  Signal         | Global Clock   | Location
  -------------------------------------------
  TFT_clk_d      | PRIMARY        |  TR BR
  loc_clk50m     | PRIMARY        |  TR TL BR BL
  loc_clk200m    | PRIMARY        |  TR TL
  loc_clk165m    | PRIMARY        |  BR BL
  sobel/shift_register_2taps/clk_ce| PRIMARY        |  TR TL BL BR
  ddr3_ctrl_2port/ui_clk| PRIMARY        |  TR TL BR
  reset_n_d      | LW             |  -
  Disp_DE_pre    | LW             |  -
  led_d_6[1]     | LW             |  -
  image_stitche_x/correct_set_pro.image1_buffer/fifo_inst/reset_r[1]| LW             |  -
  image_stitche_x/correct_set_pro.image2_buffer/fifo_inst/reset_r[1]| LW             |  -
  ddr3_ctrl_2port/fifo_ddr3_adapter/rd_data_fifo/fifo_inst/reset_r[1]| LW             |  -
  ddr3_ctrl_2port/fifo_ddr3_adapter/wr_data_fifo/fifo_inst/reset_r[1]| LW             |  -
  ddr3_ctrl_2port/your_instance_name/gw3_top/ui_clk_sync_rst| LW             |  -
  ===========================================


7. Pinout by Port Name

----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------
Port Name            | Diff Pair | Loc./Bank     | Constraint | Dir.  | Site     | IO Type    | Drive | Pull Mode | PCI Clamp | Hysteresis | Open Drain | Vref       | Single Resistor | Diff Resistor | BankVccio  | Pull Strength
----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------
clk50m               |           | T9/4          | Y          | in    | IOB29[A] | LVCMOS33   | OFF   | NONE      | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
reset_n              |           | B16/1         | Y          | in    | IOT91[A] | SSTL15_I   | OFF   | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5        | MEDIUM       
key_in0              |           | A15/1         | Y          | in    | IOT87[B] | SSTL15_I   | OFF   | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5        | MEDIUM       
uart_rx              |           | U8/5          | Y          | in    | IOB22[A] | LVCMOS33   | OFF   | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
led[0]               |           | D14/1         | Y          | out   | IOT89[A] | SSTL15_I   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5        | MEDIUM       
led[1]               |           | C14/1         | Y          | out   | IOT89[B] | SSTL15_I   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5        | MEDIUM       
led[2]               |           | B9/0          | Y          | out   | IOT58[A] | SSTL15_I   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5        | MEDIUM       
TFT_rgb[0]           |           | M18/3         | Y          | out   | IOB81[B] | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
TFT_rgb[1]           |           | M16/3         | Y          | out   | IOB81[A] | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
TFT_rgb[2]           |           | N16/3         | Y          | out   | IOB75[B] | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
TFT_rgb[3]           |           | N15/3         | Y          | out   | IOB75[A] | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
TFT_rgb[4]           |           | N14/3         | Y          | out   | IOB69[B] | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
TFT_rgb[5]           |           | H15/2         | Y          | out   | IOR24[A] | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
TFT_rgb[6]           |           | J16/3         | Y          | out   | IOB87[A] | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
TFT_rgb[7]           |           | M13/3         | Y          | out   | IOB67[B] | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
TFT_rgb[8]           |           | L14/3         | Y          | out   | IOB67[A] | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
TFT_rgb[9]           |           | L16/3         | Y          | out   | IOB91[B] | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
TFT_rgb[10]          |           | L15/3         | Y          | out   | IOB91[A] | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
TFT_rgb[11]          |           | E18/2         | Y          | out   | IOR16[B] | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
TFT_rgb[12]          |           | F16/2         | Y          | out   | IOR14[B] | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
TFT_rgb[13]          |           | F15/2         | Y          | out   | IOR14[A] | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
TFT_rgb[14]          |           | G13/2         | Y          | out   | IOR5[B]  | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
TFT_rgb[15]          |           | H12/2         | Y          | out   | IOR5[A]  | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
TFT_hs               |           | T18/3         | Y          | out   | IOB73[B] | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
TFT_vs               |           | T17/3         | Y          | out   | IOB73[A] | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
TFT_clk              |           | M14/3         | Y          | out   | IOB69[A] | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
TFT_de               |           | U18/3         | Y          | out   | IOB71[B] | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
TFT_pwm              |           | U17/3         | Y          | out   | IOB71[A] | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
hdmi_clk_p           |           | M10/5         | Y          | out   | IOB26[A] | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
hdmi_clk_n           |           | N9/5          | Y          | out   | IOB26[B] | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
hdmi_dat_p[0]        |           | R7/5          | Y          | out   | IOB6[A]  | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
hdmi_dat_p[1]        |           | T6/5          | Y          | out   | IOB16[A] | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
hdmi_dat_p[2]        |           | R5/5          | Y          | out   | IOB12[A] | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
hdmi_dat_n[0]        |           | T7/5          | Y          | out   | IOB6[B]  | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
hdmi_dat_n[1]        |           | V6/5          | Y          | out   | IOB16[B] | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
hdmi_dat_n[2]        |           | T5/5          | Y          | out   | IOB12[B] | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
uart_rx_flag         |           | F14/2         | Y          | out   | IOR7[A]  | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
uart_data_img[0]     |           | F18/2         | Y          | out   | IOR20[B] | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
uart_data_img[1]     |           | F17/2         | Y          | out   | IOR20[A] | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
uart_data_img[2]     |           | H13/2         | Y          | out   | IOR18[A] | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
uart_data_img[3]     |           | G14/2         | Y          | out   | IOR7[B]  | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
uart_data_img[4]     |           | D17/2         | Y          | out   | IOR12[A] | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
uart_data_img[5]     |           | D18/2         | Y          | out   | IOR12[B] | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
uart_data_img[6]     |           | G16/2         | Y          | out   | IOR22[A] | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
uart_data_img[7]     |           | G18/2         | Y          | out   | IOR22[B] | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
uart_byte_vaild_r0   |           | C17/2         | Y          | out   | IOR9[A]  | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
image_data_valid_r0  |           | C18/2         | Y          | out   | IOR9[B]  | LVCMOS33   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3        | MEDIUM       
O_ddr_addr[0]        |           | A3/0          | Y          | out   | IOT35[B] | SSTL15_I   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5        | MEDIUM       
O_ddr_addr[1]        |           | A6/0          | Y          | out   | IOT43[B] | SSTL15_I   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5        | MEDIUM       
O_ddr_addr[2]        |           | B3/0          | Y          | out   | IOT35[A] | SSTL15_I   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5        | MEDIUM       
O_ddr_addr[3]        |           | C7/0          | Y          | out   | IOT48[A] | SSTL15_I   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5        | MEDIUM       
O_ddr_addr[4]        |           | B4/0          | Y          | out   | IOT37[A] | SSTL15_I   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5        | MEDIUM       
O_ddr_addr[5]        |           | C8/0          | Y          | out   | IOT50[B] | SSTL15_I   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5        | MEDIUM       
O_ddr_addr[6]        |           | C4/0          | Y          | out   | IOT29[B] | SSTL15_I   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5        | MEDIUM       
O_ddr_addr[7]        |           | C6/0          | Y          | out   | IOT33[B] | SSTL15_I   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5        | MEDIUM       
O_ddr_addr[8]        |           | D4/0          | Y          | out   | IOT29[A] | SSTL15_I   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5        | MEDIUM       
O_ddr_addr[9]        |           | A2/0          | Y          | out   | IOT31[B] | SSTL15_I   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5        | MEDIUM       
O_ddr_addr[10]       |           | E6/0          | Y          | out   | IOT41[B] | SSTL15_I   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5        | MEDIUM       
O_ddr_addr[11]       |           | B6/0          | Y          | out   | IOT43[A] | SSTL15_I   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5        | MEDIUM       
O_ddr_addr[12]       |           | A5/0          | Y          | out   | IOT39[B] | SSTL15_I   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5        | MEDIUM       
O_ddr_addr[13]       |           | B2/0          | Y          | out   | IOT31[A] | SSTL15_I   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5        | MEDIUM       
O_ddr_ba[0]          |           | D6/0          | Y          | out   | IOT33[A] | SSTL15_I   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5        | MEDIUM       
O_ddr_ba[1]          |           | A4/0          | Y          | out   | IOT37[B] | SSTL15_I   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5        | MEDIUM       
O_ddr_ba[2]          |           | D8/0          | Y          | out   | IOT50[A] | SSTL15_I   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5        | MEDIUM       
O_ddr_cs_n           |           | E7/0          | Y          | out   | IOT45[A] | SSTL15_I   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5        | MEDIUM       
O_ddr_ras_n          |           | G8/0          | Y          | out   | IOT52[A] | SSTL15_I   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5        | MEDIUM       
O_ddr_cas_n          |           | F8/0          | Y          | out   | IOT52[B] | SSTL15_I   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5        | MEDIUM       
O_ddr_we_n           |           | E8/0          | Y          | out   | IOT45[B] | SSTL15_I   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5        | MEDIUM       
O_ddr_clk            | O_ddr_clk_n | D9,C9/0       | Y          | out   | IOT56    | SSTL15D_I  | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5        | MEDIUM       
O_ddr_cke            |           | C5/0          | Y          | out   | IOT39[A] | SSTL15_I   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5        | MEDIUM       
O_ddr_odt            |           | F7/0          | Y          | out   | IOT41[A] | SSTL15_I   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5        | MEDIUM       
O_ddr_reset_n        |           | A7/0          | Y          | out   | IOT48[B] | SSTL15_I   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5        | MEDIUM       
O_ddr_dqm[0]         |           | F9/1          | Y          | out   | IOT66[B] | SSTL15_I   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5        | MEDIUM       
O_ddr_dqm[1]         |           | F13/1         | Y          | out   | IOT85[A] | SSTL15_I   | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5        | MEDIUM       
IO_ddr_dq[0]         |           | A12/1         | Y          | io    | IOT72[B] | SSTL15_I   | 8     | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5        | MEDIUM       
IO_ddr_dq[1]         |           | B11/1         | Y          | io    | IOT68[A] | SSTL15_I   | 8     | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5        | MEDIUM       
IO_ddr_dq[2]         |           | G9/1          | Y          | io    | IOT66[A] | SSTL15_I   | 8     | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5        | MEDIUM       
IO_ddr_dq[3]         |           | G11/1         | Y          | io    | IOT70[A] | SSTL15_I   | 8     | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5        | MEDIUM       
IO_ddr_dq[4]         |           | A11/1         | Y          | io    | IOT68[B] | SSTL15_I   | 8     | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5        | MEDIUM       
IO_ddr_dq[5]         |           | C10/1         | Y          | io    | IOT63[A] | SSTL15_I   | 8     | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5        | MEDIUM       
IO_ddr_dq[6]         |           | F10/1         | Y          | io    | IOT70[B] | SSTL15_I   | 8     | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5        | MEDIUM       
IO_ddr_dq[7]         |           | A10/1         | Y          | io    | IOT63[B] | SSTL15_I   | 8     | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5        | MEDIUM       
IO_ddr_dq[8]         |           | C13/1         | Y          | io    | IOT78[A] | SSTL15_I   | 8     | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5        | MEDIUM       
IO_ddr_dq[9]         |           | A13/1         | Y          | io    | IOT78[B] | SSTL15_I   | 8     | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5        | MEDIUM       
IO_ddr_dq[10]        |           | E11/1         | Y          | io    | IOT74[B] | SSTL15_I   | 8     | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5        | MEDIUM       
IO_ddr_dq[11]        |           | F11/1         | Y          | io    | IOT74[A] | SSTL15_I   | 8     | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5        | MEDIUM       
IO_ddr_dq[12]        |           | C12/1         | Y          | io    | IOT76[B] | SSTL15_I   | 8     | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5        | MEDIUM       
IO_ddr_dq[13]        |           | D12/1         | Y          | io    | IOT76[A] | SSTL15_I   | 8     | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5        | MEDIUM       
IO_ddr_dq[14]        |           | B14/1         | Y          | io    | IOT83[A] | SSTL15_I   | 8     | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5        | MEDIUM       
IO_ddr_dq[15]        |           | A14/1         | Y          | io    | IOT83[B] | SSTL15_I   | 8     | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5        | MEDIUM       
IO_ddr_dqs[0]        | IO_ddr_dqs_n[0] | D11,C11/1     | Y          | io    | IOT61    | SSTL15D_I  | 8     | NONE      | OFF       | NONE       | OFF        | OFF        | OFF             | OFF           | 1.5        | MEDIUM       
IO_ddr_dqs[1]        | IO_ddr_dqs_n[1] | F12,E12/1     | Y          | io    | IOT80    | SSTL15D_I  | 8     | NONE      | OFF       | NONE       | OFF        | OFF        | OFF             | OFF           | 1.5        | MEDIUM       
============================================================================================================================================================================================================================




8. All Package Pins

-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------
Loc./Bank| Signal               | Dir.  | Site     | IO Type  | Drive | Pull Mode | PCI Clamp | Hysteresis | Open Drain | Vref       | Single Resistor | Diff Resistor | Bank Vccio | Pull Strength
-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------
H4/7     | -                    | in    | IOT1[A]  | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
H3/7     | -                    | in    | IOT1[B]  | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
L5/7     | -                    | in    | IOT3[A]  | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
K5/7     | -                    | in    | IOT3[B]  | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
H5/7     | -                    | in    | IOT5[B]  | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
G3/7     | -                    | in    | IOT7[A]  | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
G1/7     | -                    | in    | IOT7[B]  | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
H7/7     | -                    | in    | IOT9[A]  | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
G6/7     | -                    | in    | IOT9[B]  | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
F2/7     | -                    | in    | IOT11[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
F1/7     | -                    | in    | IOT11[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
J7/7     | -                    | in    | IOT13[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
J6/7     | -                    | in    | IOT13[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
E3/7     | -                    | in    | IOT15[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
E1/7     | -                    | in    | IOT15[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
F4/7     | -                    | in    | IOT17[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
F3/7     | -                    | in    | IOT17[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
D2/7     | -                    | in    | IOT19[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
D1/7     | -                    | in    | IOT19[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
L7/7     | -                    | in    | IOT21[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
K6/7     | -                    | in    | IOT21[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
E4/7     | -                    | in    | IOT23[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
D3/7     | -                    | in    | IOT23[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
F6/7     | -                    | in    | IOT25[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
F5/7     | -                    | in    | IOT25[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
C2/7     | -                    | in    | IOT27[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
C1/7     | -                    | in    | IOT27[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
D4/0     | O_ddr_addr[8]        | out   | IOT29[A] | SSTL15_I | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
C4/0     | O_ddr_addr[6]        | out   | IOT29[B] | SSTL15_I | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
B2/0     | O_ddr_addr[13]       | out   | IOT31[A] | SSTL15_I | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
A2/0     | O_ddr_addr[9]        | out   | IOT31[B] | SSTL15_I | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
D6/0     | O_ddr_ba[0]          | out   | IOT33[A] | SSTL15_I | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
C6/0     | O_ddr_addr[7]        | out   | IOT33[B] | SSTL15_I | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
B3/0     | O_ddr_addr[2]        | out   | IOT35[A] | SSTL15_I | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
A3/0     | O_ddr_addr[0]        | out   | IOT35[B] | SSTL15_I | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
B4/0     | O_ddr_addr[4]        | out   | IOT37[A] | SSTL15_I | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
A4/0     | O_ddr_ba[1]          | out   | IOT37[B] | SSTL15_I | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
C5/0     | O_ddr_cke            | out   | IOT39[A] | SSTL15_I | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
A5/0     | O_ddr_addr[12]       | out   | IOT39[B] | SSTL15_I | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
F7/0     | O_ddr_odt            | out   | IOT41[A] | SSTL15_I | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
E6/0     | O_ddr_addr[10]       | out   | IOT41[B] | SSTL15_I | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
B6/0     | O_ddr_addr[11]       | out   | IOT43[A] | SSTL15_I | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
A6/0     | O_ddr_addr[1]        | out   | IOT43[B] | SSTL15_I | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
E7/0     | O_ddr_cs_n           | out   | IOT45[A] | SSTL15_I | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
E8/0     | O_ddr_we_n           | out   | IOT45[B] | SSTL15_I | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
C7/0     | O_ddr_addr[3]        | out   | IOT48[A] | SSTL15_I | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
A7/0     | O_ddr_reset_n        | out   | IOT48[B] | SSTL15_I | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
D8/0     | O_ddr_ba[2]          | out   | IOT50[A] | SSTL15_I | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
C8/0     | O_ddr_addr[5]        | out   | IOT50[B] | SSTL15_I | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
G8/0     | O_ddr_ras_n          | out   | IOT52[A] | SSTL15_I | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
F8/0     | O_ddr_cas_n          | out   | IOT52[B] | SSTL15_I | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
B8/0     | -                    | in    | IOT54[A] | LVCMOS15 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
A8/0     | -                    | in    | IOT54[B] | LVCMOS15 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
D9/0     | O_ddr_clk            | out   | IOT56[A] | SSTL15D_I | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
C9/0     | O_ddr_clk_n          | out   | IOT56[B] | SSTL15D_I | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
B9/0     | led[2]               | out   | IOT58[A] | SSTL15_I | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
A9/0     | -                    | in    | IOT58[B] | LVCMOS15 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
D11/1    | IO_ddr_dqs[0]        | io    | IOT61[A] | SSTL15D_I | 8     | NONE      | OFF       | NONE       | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
C11/1    | IO_ddr_dqs_n[0]      | io    | IOT61[B] | SSTL15D_I | 8     | NONE      | OFF       | NONE       | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
C10/1    | IO_ddr_dq[5]         | io    | IOT63[A] | SSTL15_I | 8     | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5   | MEDIUM       
A10/1    | IO_ddr_dq[7]         | io    | IOT63[B] | SSTL15_I | 8     | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5   | MEDIUM       
G9/1     | IO_ddr_dq[2]         | io    | IOT66[A] | SSTL15_I | 8     | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5   | MEDIUM       
F9/1     | O_ddr_dqm[0]         | out   | IOT66[B] | SSTL15_I | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
B11/1    | IO_ddr_dq[1]         | io    | IOT68[A] | SSTL15_I | 8     | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5   | MEDIUM       
A11/1    | IO_ddr_dq[4]         | io    | IOT68[B] | SSTL15_I | 8     | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5   | MEDIUM       
G11/1    | IO_ddr_dq[3]         | io    | IOT70[A] | SSTL15_I | 8     | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5   | MEDIUM       
F10/1    | IO_ddr_dq[6]         | io    | IOT70[B] | SSTL15_I | 8     | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5   | MEDIUM       
A12/1    | IO_ddr_dq[0]         | io    | IOT72[B] | SSTL15_I | 8     | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5   | MEDIUM       
F11/1    | IO_ddr_dq[11]        | io    | IOT74[A] | SSTL15_I | 8     | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5   | MEDIUM       
E11/1    | IO_ddr_dq[10]        | io    | IOT74[B] | SSTL15_I | 8     | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5   | MEDIUM       
D12/1    | IO_ddr_dq[13]        | io    | IOT76[A] | SSTL15_I | 8     | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5   | MEDIUM       
C12/1    | IO_ddr_dq[12]        | io    | IOT76[B] | SSTL15_I | 8     | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5   | MEDIUM       
C13/1    | IO_ddr_dq[8]         | io    | IOT78[A] | SSTL15_I | 8     | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5   | MEDIUM       
A13/1    | IO_ddr_dq[9]         | io    | IOT78[B] | SSTL15_I | 8     | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5   | MEDIUM       
F12/1    | IO_ddr_dqs[1]        | io    | IOT80[A] | SSTL15D_I | 8     | NONE      | OFF       | NONE       | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
E12/1    | IO_ddr_dqs_n[1]      | io    | IOT80[B] | SSTL15D_I | 8     | NONE      | OFF       | NONE       | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
B14/1    | IO_ddr_dq[14]        | io    | IOT83[A] | SSTL15_I | 8     | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5   | MEDIUM       
A14/1    | IO_ddr_dq[15]        | io    | IOT83[B] | SSTL15_I | 8     | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5   | MEDIUM       
F13/1    | O_ddr_dqm[1]         | out   | IOT85[A] | SSTL15_I | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
E13/1    | -                    | in    | IOT85[B] | LVCMOS15 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
C15/1    | -                    | in    | IOT87[A] | LVCMOS15 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
A15/1    | key_in0              | in    | IOT87[B] | SSTL15_I | OFF   | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5   | MEDIUM       
D14/1    | led[0]               | out   | IOT89[A] | SSTL15_I | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
C14/1    | led[1]               | out   | IOT89[B] | SSTL15_I | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
B16/1    | reset_n              | in    | IOT91[A] | SSTL15_I | OFF   | NONE      | OFF       | NONE       | OFF        | INTERNAL   | OFF             | OFF           | 1.5   | MEDIUM       
A16/1    | -                    | in    | IOT91[B] | LVCMOS15 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 1.5   | MEDIUM       
-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------
V2/5     | -                    | in    | IOB1[A]  | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
T4/5     | -                    | in    | IOB2[A]  | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
N5/5     | -                    | in    | IOB4[A]  | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
P6/5     | -                    | in    | IOB4[B]  | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
R7/5     | hdmi_dat_p[0]        | out   | IOB6[A]  | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
T7/5     | hdmi_dat_n[0]        | out   | IOB6[B]  | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
R3/5     | -                    | in    | IOB8[A]  | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
T3/5     | -                    | in    | IOB8[B]  | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
U5/5     | -                    | in    | IOB10[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
V5/5     | -                    | in    | IOB10[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
R5/5     | hdmi_dat_p[2]        | out   | IOB12[A] | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
T5/5     | hdmi_dat_n[2]        | out   | IOB12[B] | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
N6/5     | -                    | in    | IOB14[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
P7/5     | -                    | in    | IOB14[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
T6/5     | hdmi_dat_p[1]        | out   | IOB16[A] | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
V6/5     | hdmi_dat_n[1]        | out   | IOB16[B] | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
P8/5     | -                    | in    | IOB18[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
U7/5     | -                    | in    | IOB20[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
V7/5     | -                    | in    | IOB20[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
U8/5     | uart_rx              | in    | IOB22[A] | LVCMOS33 | OFF   | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
V8/5     | -                    | in    | IOB22[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
M8/5     | -                    | in    | IOB24[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
N8/5     | -                    | in    | IOB24[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
M10/5    | hdmi_clk_p           | out   | IOB26[A] | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
N9/5     | hdmi_clk_n           | out   | IOB26[B] | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
T9/4     | clk50m               | in    | IOB29[A] | LVCMOS33 | OFF   | NONE      | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
V9/4     | -                    | in    | IOB29[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
R8/4     | -                    | in    | IOB31[A] | LVCMOS33 | 8     | NONE      | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
T8/4     | -                    | in    | IOB31[B] | LVCMOS33 | 8     | NONE      | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
U10/4    | -                    | in    | IOB33[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
V10/4    | -                    | in    | IOB33[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
R10/4    | -                    | in    | IOB35[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
T10/4    | -                    | in    | IOB35[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
U3/4     | -                    | in    | IOB37[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
V3/4     | -                    | in    | IOB37[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
U11/4    | -                    | in    | IOB39[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
V11/4    | -                    | in    | IOB39[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
N10/4    | -                    | in    | IOB41[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
P11/4    | -                    | in    | IOB41[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
T12/4    | -                    | in    | IOB43[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
V12/4    | -                    | in    | IOB43[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
R11/4    | -                    | in    | IOB45[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
T11/4    | -                    | in    | IOB45[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
M11/4    | -                    | in    | IOB48[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
N11/4    | -                    | in    | IOB48[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
U13/4    | -                    | in    | IOB50[A] | LVCMOS33 | 8     | NONE      | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
V13/4    | -                    | in    | IOB50[B] | LVCMOS33 | 8     | NONE      | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
N12/4    | -                    | in    | IOB52[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
P12/4    | -                    | in    | IOB52[B] | LVCMOS33 | 8     | NONE      | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
T14/4    | -                    | in    | IOB54[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
V14/4    | -                    | in    | IOB54[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
U15/4    | -                    | in    | IOB56[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
V15/4    | -                    | in    | IOB56[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
R13/4    | -                    | in    | IOB58[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
T13/4    | -                    | in    | IOB58[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
U16/4    | -                    | in    | IOB60[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
V16/4    | -                    | in    | IOB60[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
R15/4    | -                    | in    | IOB62[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
T15/4    | -                    | in    | IOB62[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
V17/4    | -                    | in    | IOB64[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
P15/3    | -                    | in    | IOB65[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
P16/3    | -                    | in    | IOB65[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
L14/3    | TFT_rgb[8]           | out   | IOB67[A] | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
M13/3    | TFT_rgb[7]           | out   | IOB67[B] | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
M14/3    | TFT_clk              | out   | IOB69[A] | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
N14/3    | TFT_rgb[4]           | out   | IOB69[B] | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
U17/3    | TFT_pwm              | out   | IOB71[A] | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
U18/3    | TFT_de               | out   | IOB71[B] | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
T17/3    | TFT_vs               | out   | IOB73[A] | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
T18/3    | TFT_hs               | out   | IOB73[B] | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
N15/3    | TFT_rgb[3]           | out   | IOB75[A] | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
N16/3    | TFT_rgb[2]           | out   | IOB75[B] | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
P17/3    | -                    | in    | IOB77[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
P18/3    | -                    | in    | IOB77[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
N17/3    | -                    | in    | IOB79[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
N18/3    | -                    | in    | IOB79[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
M16/3    | TFT_rgb[1]           | out   | IOB81[A] | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
M18/3    | TFT_rgb[0]           | out   | IOB81[B] | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
L17/3    | -                    | in    | IOB83[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
L18/3    | -                    | in    | IOB83[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
K17/3    | -                    | in    | IOB85[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
K18/3    | -                    | in    | IOB85[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
J16/3    | TFT_rgb[6]           | out   | IOB87[A] | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
H17/3    | -                    | in    | IOB89[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
H18/3    | -                    | in    | IOB89[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
L15/3    | TFT_rgb[10]          | out   | IOB91[A] | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
L16/3    | TFT_rgb[9]           | out   | IOB91[B] | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------
H2/6     | -                    | in    | IOL3[A]  | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
H1/6     | -                    | in    | IOL3[B]  | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
K4/6     | -                    | in    | IOL5[A]  | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
K3/6     | -                    | in    | IOL5[B]  | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
J1/6     | -                    | in    | IOL7[B]  | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
L4/6     | -                    | in    | IOL9[A]  | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
L3/6     | -                    | in    | IOL9[B]  | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
K2/6     | -                    | in    | IOL12[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
K1/6     | -                    | in    | IOL12[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
L2/6     | -                    | in    | IOL14[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
L1/6     | -                    | in    | IOL14[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
M3/6     | -                    | in    | IOL16[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
M1/6     | -                    | in    | IOL16[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
N2/6     | -                    | in    | IOL18[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
N1/6     | -                    | in    | IOL18[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
P2/6     | -                    | in    | IOL21[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
P1/6     | -                    | in    | IOL21[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------
A17/10   | -                    | in    | IOR1[A]  | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
D15/10   | -                    | in    | IOR1[B]  | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
B18/10   | -                    | in    | IOR3[A]  | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
D16/10   | -                    | out   | IOR3[B]  | LVCMOS33 | 8     | UP        | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
H12/2    | TFT_rgb[15]          | out   | IOR5[A]  | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
G13/2    | TFT_rgb[14]          | out   | IOR5[B]  | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
F14/2    | uart_rx_flag         | out   | IOR7[A]  | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
G14/2    | uart_data_img[3]     | out   | IOR7[B]  | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
C17/2    | uart_byte_vaild_r0   | out   | IOR9[A]  | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
C18/2    | image_data_valid_r0  | out   | IOR9[B]  | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
D17/2    | uart_data_img[4]     | out   | IOR12[A] | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
D18/2    | uart_data_img[5]     | out   | IOR12[B] | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
F15/2    | TFT_rgb[13]          | out   | IOR14[A] | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
F16/2    | TFT_rgb[12]          | out   | IOR14[B] | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
E16/2    | -                    | in    | IOR16[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
E18/2    | TFT_rgb[11]          | out   | IOR16[B] | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
H13/2    | uart_data_img[2]     | out   | IOR18[A] | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
H14/2    | -                    | in    | IOR18[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
F17/2    | uart_data_img[1]     | out   | IOR20[A] | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
F18/2    | uart_data_img[0]     | out   | IOR20[B] | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
G16/2    | uart_data_img[6]     | out   | IOR22[A] | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
G18/2    | uart_data_img[7]     | out   | IOR22[B] | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
H15/2    | TFT_rgb[5]           | out   | IOR24[A] | LVCMOS33 | 8     | NONE      | OFF       | OFF        | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
J13/2    | -                    | in    | IOR26[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
K14/2    | -                    | in    | IOR26[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
K12/2    | -                    | in    | IOR29[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
K13/2    | -                    | in    | IOR29[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
L12/2    | -                    | in    | IOR31[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
L13/2    | -                    | in    | IOR31[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
K15/2    | -                    | in    | IOR33[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
K16/2    | -                    | in    | IOR33[B] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
R16/11   | -                    | in    | IOR35[A] | LVCMOS33 | 8     | UP        | OFF       | ON         | OFF        | OFF        | OFF             | OFF           | 3.3   | MEDIUM       
-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------
=================================================================================================================================================================================================


