- PnR Messages
- PnR Details
- Resource
  - Resource Usage Summary
  - I/O Bank Usage Summary
  - Global Clock Usage Summary
  - Global Clock Signals
  - Pinout by Port Name
  - All Package Pins

# PnR Messages

Report Title | PnR Report
Design File | H:\01_gaoyun\gao_project\60_uart_ddr3_tft_hdmi_sobel_filter\uart_ddr3_tft_hdmi_sobel_filter\impl\gwsynthesis\uart_ddr3_tft_hdmi_sobel_filter.vg
Physical Constraints File | H:\01_gaoyun\gao_project\60_uart_ddr3_tft_hdmi_sobel_filter\uart_ddr3_tft_hdmi_sobel_filter\src\uart_ddr3_tft_hdmi_sobel_filter.cst
Timing Constraints File | ---
Version | V1.9.9 Beta-3
Part Number | GW5A-LV25UG324ES
Device | GW5A-25
Device Version | A
Created Time | Wed Aug 30 14:39:15 2023
Legal Announcement | Copyright (C)2014-2023 Gowin Semiconductor Corporation. All rights reserved.

# PnR Details

Place & Route Process | Running placement: Placement Phase 0: CPU time = 0h 0m 4s, Elapsed time = 0h 0m 4s Placement Phase 1: CPU time = 0h 0m 0.515s, Elapsed time = 0h 0m 0.515s Placement Phase 2: CPU time = 0h 0m 23s, Elapsed time = 0h 0m 23s Placement Phase 3: CPU time = 0h 0m 34s, Elapsed time = 0h 0m 34s Total Placement: CPU time = 0h 1m 1s, Elapsed time = 0h 1m 1s Running routing: Routing Phase 0: CPU time = 0h 0m 0.006s, Elapsed time = 0h 0m 0.005s Routing Phase 1: CPU time = 0h 0m 29s, Elapsed time = 0h 0m 29s Routing Phase 2: CPU time = 0h 0m 0.219s, Elapsed time = 0h 0m 0.218s Routing Phase 3: CPU time = 0h 0m 0s, Elapsed time = 0h 0m 0s Total Routing: CPU time = 0h 0m 29s, Elapsed time = 0h 0m 29s Generate output files: CPU time = 0h 0m 3s, Elapsed time = 0h 0m 3s
Total Time and Memory Usage | CPU time = 0h 1m 34s, Elapsed time = 0h 1m 34s, Peak memory usage = 527MB

# Resource

## Resource Usage Summary:

Resource | Usage | Utilization
Logic | 10153/23040 | 45%
--LUT,ALU,ROM16 | 10081(9480 LUT, 601 ALU, 0 ROM16) | -
--SSRAM(RAM16) | 12 | -
Register | 12077/23685 | 51%
--Logic Register as Latch | 0/23040 | 0%
--Logic Register as FF | 12075/23040 | 53%
--I/O Register as Latch | 0/645 | 0%
--I/O Register as FF | 2/645 | <1%
CLS | 10569/11520 | 92%
I/O Port | 95 | -
I/O Buf | 92 | -
--Input Buf | 4 | -
--Output Buf | 70 | -
--Inout Buf | 18 | -
IOLOGIC | 8 ODDR 16 IDES8_MEM 24 OSER8 20 OSER8_MEM 16 IODELAY | 60%
BSRAM | 14 SDPB 8 SDPX9B | 40%
DSP | 0 | 0%
PLL | 2/6 | 34%
DDRDLL | 1/4 | 25%
DCS | 0/8 | 0%
DQCE | 1/24 | 5%
OSC | 0/1 | 0%
CLKDIV | 2/16 | 13%
DLLDLY | 0/8 | 0%
DQS | 2/8 | 25%
DHCEN | 1/16 | 7%

## I/O Bank Usage Summary:

I/O Bank | Usage
bank 0 | 27/30(90%)
bank 1 | 26/29(89%)
bank 2 | 17/27(62%)
bank 3 | 15/27(55%)
bank 4 | 1/35(2%)
bank 5 | 9/25(36%)
bank 6 | 0/17(0%)
bank 7 | 0/27(0%)
bank 10 | 0/4(0%)

## Global Clock Usage Summary:

Global Clock | Usage
PRIMARY | 6/8(75%)
LW | 8/8(100%)
GCLK_PIN | 9/20(45%)
PLL | 0/6(0%)
DDRDLL | 1/4(25%)
CLKDIV | 2/16(13%)
DLLDLY | 0/8(0%)

## Global Clock Signals:

Signal | Global Clock | Location
TFT_clk_d | PRIMARY | TR BR
loc_clk50m | PRIMARY | TR TL BR BL
loc_clk200m | PRIMARY | TR TL
loc_clk165m | PRIMARY | BR BL
sobel/shift_register_2taps/clk_ce | PRIMARY | TR TL BL BR
ddr3_ctrl_2port/ui_clk | PRIMARY | TR TL BR
reset_n_d | LW | -
Disp_DE_pre | LW | -
led_d_6[1] | LW | -
image_stitche_x/correct_set_pro.image1_buffer/fifo_inst/reset_r[1] | LW | -
image_stitche_x/correct_set_pro.image2_buffer/fifo_inst/reset_r[1] | LW | -
ddr3_ctrl_2port/fifo_ddr3_adapter/rd_data_fifo/fifo_inst/reset_r[1] | LW | -
ddr3_ctrl_2port/fifo_ddr3_adapter/wr_data_fifo/fifo_inst/reset_r[1] | LW | -
ddr3_ctrl_2port/your_instance_name/gw3_top/ui_clk_sync_rst | LW | -

## Pinout by Port Name:

Port Name | Diff Pair | Loc./Bank | Constraint | Dir. | Site | IO Type | Drive | Pull Mode | PCI Clamp | Hysteresis | Open Drain | Vref | Single Resistor | Diff Resistor | BankVccio | Pull Strength
clk50m |  | T9/4 | Y | in | IOB29[A] | LVCMOS33 | OFF | NONE | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
reset_n |  | B16/1 | Y | in | IOT91[A] | SSTL15_I | OFF | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
key_in0 |  | A15/1 | Y | in | IOT87[B] | SSTL15_I | OFF | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
uart_rx |  | U8/5 | Y | in | IOB22[A] | LVCMOS33 | OFF | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
led[0] |  | D14/1 | Y | out | IOT89[A] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
led[1] |  | C14/1 | Y | out | IOT89[B] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
led[2] |  | B9/0 | Y | out | IOT58[A] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
TFT_rgb[0] |  | M18/3 | Y | out | IOB81[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
TFT_rgb[1] |  | M16/3 | Y | out | IOB81[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
TFT_rgb[2] |  | N16/3 | Y | out | IOB75[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
TFT_rgb[3] |  | N15/3 | Y | out | IOB75[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
TFT_rgb[4] |  | N14/3 | Y | out | IOB69[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
TFT_rgb[5] |  | H15/2 | Y | out | IOR24[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
TFT_rgb[6] |  | J16/3 | Y | out | IOB87[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
TFT_rgb[7] |  | M13/3 | Y | out | IOB67[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
TFT_rgb[8] |  | L14/3 | Y | out | IOB67[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
TFT_rgb[9] |  | L16/3 | Y | out | IOB91[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
TFT_rgb[10] |  | L15/3 | Y | out | IOB91[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
TFT_rgb[11] |  | E18/2 | Y | out | IOR16[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
TFT_rgb[12] |  | F16/2 | Y | out | IOR14[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
TFT_rgb[13] |  | F15/2 | Y | out | IOR14[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
TFT_rgb[14] |  | G13/2 | Y | out | IOR5[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
TFT_rgb[15] |  | H12/2 | Y | out | IOR5[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
TFT_hs |  | T18/3 | Y | out | IOB73[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
TFT_vs |  | T17/3 | Y | out | IOB73[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
TFT_clk |  | M14/3 | Y | out | IOB69[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
TFT_de |  | U18/3 | Y | out | IOB71[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
TFT_pwm |  | U17/3 | Y | out | IOB71[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
hdmi_clk_p |  | M10/5 | Y | out | IOB26[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
hdmi_clk_n |  | N9/5 | Y | out | IOB26[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
hdmi_dat_p[0] |  | R7/5 | Y | out | IOB6[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
hdmi_dat_p[1] |  | T6/5 | Y | out | IOB16[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
hdmi_dat_p[2] |  | R5/5 | Y | out | IOB12[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
hdmi_dat_n[0] |  | T7/5 | Y | out | IOB6[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
hdmi_dat_n[1] |  | V6/5 | Y | out | IOB16[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
hdmi_dat_n[2] |  | T5/5 | Y | out | IOB12[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
uart_rx_flag |  | F14/2 | Y | out | IOR7[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
uart_data_img[0] |  | F18/2 | Y | out | IOR20[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
uart_data_img[1] |  | F17/2 | Y | out | IOR20[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
uart_data_img[2] |  | H13/2 | Y | out | IOR18[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
uart_data_img[3] |  | G14/2 | Y | out | IOR7[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
uart_data_img[4] |  | D17/2 | Y | out | IOR12[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
uart_data_img[5] |  | D18/2 | Y | out | IOR12[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
uart_data_img[6] |  | G16/2 | Y | out | IOR22[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
uart_data_img[7] |  | G18/2 | Y | out | IOR22[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
uart_byte_vaild_r0 |  | C17/2 | Y | out | IOR9[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
image_data_valid_r0 |  | C18/2 | Y | out | IOR9[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
O_ddr_addr[0] |  | A3/0 | Y | out | IOT35[B] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
O_ddr_addr[1] |  | A6/0 | Y | out | IOT43[B] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
O_ddr_addr[2] |  | B3/0 | Y | out | IOT35[A] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
O_ddr_addr[3] |  | C7/0 | Y | out | IOT48[A] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
O_ddr_addr[4] |  | B4/0 | Y | out | IOT37[A] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
O_ddr_addr[5] |  | C8/0 | Y | out | IOT50[B] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
O_ddr_addr[6] |  | C4/0 | Y | out | IOT29[B] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
O_ddr_addr[7] |  | C6/0 | Y | out | IOT33[B] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
O_ddr_addr[8] |  | D4/0 | Y | out | IOT29[A] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
O_ddr_addr[9] |  | A2/0 | Y | out | IOT31[B] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
O_ddr_addr[10] |  | E6/0 | Y | out | IOT41[B] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
O_ddr_addr[11] |  | B6/0 | Y | out | IOT43[A] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
O_ddr_addr[12] |  | A5/0 | Y | out | IOT39[B] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
O_ddr_addr[13] |  | B2/0 | Y | out | IOT31[A] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
O_ddr_ba[0] |  | D6/0 | Y | out | IOT33[A] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
O_ddr_ba[1] |  | A4/0 | Y | out | IOT37[B] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
O_ddr_ba[2] |  | D8/0 | Y | out | IOT50[A] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
O_ddr_cs_n |  | E7/0 | Y | out | IOT45[A] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
O_ddr_ras_n |  | G8/0 | Y | out | IOT52[A] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
O_ddr_cas_n |  | F8/0 | Y | out | IOT52[B] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
O_ddr_we_n |  | E8/0 | Y | out | IOT45[B] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
O_ddr_clk | O_ddr_clk_n | D9,C9/0 | Y | out | IOT56 | SSTL15D_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
O_ddr_cke |  | C5/0 | Y | out | IOT39[A] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
O_ddr_odt |  | F7/0 | Y | out | IOT41[A] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
O_ddr_reset_n |  | A7/0 | Y | out | IOT48[B] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
O_ddr_dqm[0] |  | F9/1 | Y | out | IOT66[B] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
O_ddr_dqm[1] |  | F13/1 | Y | out | IOT85[A] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
IO_ddr_dq[0] |  | A12/1 | Y | io | IOT72[B] | SSTL15_I | 8 | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
IO_ddr_dq[1] |  | B11/1 | Y | io | IOT68[A] | SSTL15_I | 8 | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
IO_ddr_dq[2] |  | G9/1 | Y | io | IOT66[A] | SSTL15_I | 8 | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
IO_ddr_dq[3] |  | G11/1 | Y | io | IOT70[A] | SSTL15_I | 8 | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
IO_ddr_dq[4] |  | A11/1 | Y | io | IOT68[B] | SSTL15_I | 8 | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
IO_ddr_dq[5] |  | C10/1 | Y | io | IOT63[A] | SSTL15_I | 8 | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
IO_ddr_dq[6] |  | F10/1 | Y | io | IOT70[B] | SSTL15_I | 8 | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
IO_ddr_dq[7] |  | A10/1 | Y | io | IOT63[B] | SSTL15_I | 8 | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
IO_ddr_dq[8] |  | C13/1 | Y | io | IOT78[A] | SSTL15_I | 8 | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
IO_ddr_dq[9] |  | A13/1 | Y | io | IOT78[B] | SSTL15_I | 8 | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
IO_ddr_dq[10] |  | E11/1 | Y | io | IOT74[B] | SSTL15_I | 8 | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
IO_ddr_dq[11] |  | F11/1 | Y | io | IOT74[A] | SSTL15_I | 8 | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
IO_ddr_dq[12] |  | C12/1 | Y | io | IOT76[B] | SSTL15_I | 8 | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
IO_ddr_dq[13] |  | D12/1 | Y | io | IOT76[A] | SSTL15_I | 8 | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
IO_ddr_dq[14] |  | B14/1 | Y | io | IOT83[A] | SSTL15_I | 8 | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
IO_ddr_dq[15] |  | A14/1 | Y | io | IOT83[B] | SSTL15_I | 8 | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
IO_ddr_dqs[0] | IO_ddr_dqs_n[0] | D11,C11/1 | Y | io | IOT61 | SSTL15D_I | 8 | NONE | OFF | NONE | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
IO_ddr_dqs[1] | IO_ddr_dqs_n[1] | F12,E12/1 | Y | io | IOT80 | SSTL15D_I | 8 | NONE | OFF | NONE | OFF | OFF | OFF | OFF | 1.5 | MEDIUM

## All Package Pins:

Loc./Bank | Signal | Dir. | Site | IO Type | Drive | Pull Mode | PCI Clamp | Hysteresis | Open Drain | Vref | Single Resistor | Diff Resistor | Bank Vccio | Pull Strength
H4/7 | - | in | IOT1[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
H3/7 | - | in | IOT1[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
L5/7 | - | in | IOT3[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
K5/7 | - | in | IOT3[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
H5/7 | - | in | IOT5[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
G3/7 | - | in | IOT7[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
G1/7 | - | in | IOT7[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
H7/7 | - | in | IOT9[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
G6/7 | - | in | IOT9[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
F2/7 | - | in | IOT11[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
F1/7 | - | in | IOT11[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
J7/7 | - | in | IOT13[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
J6/7 | - | in | IOT13[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
E3/7 | - | in | IOT15[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
E1/7 | - | in | IOT15[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
F4/7 | - | in | IOT17[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
F3/7 | - | in | IOT17[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
D2/7 | - | in | IOT19[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
D1/7 | - | in | IOT19[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
L7/7 | - | in | IOT21[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
K6/7 | - | in | IOT21[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
E4/7 | - | in | IOT23[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
D3/7 | - | in | IOT23[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
F6/7 | - | in | IOT25[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
F5/7 | - | in | IOT25[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
C2/7 | - | in | IOT27[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
C1/7 | - | in | IOT27[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
D4/0 | O_ddr_addr[8] | out | IOT29[A] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
C4/0 | O_ddr_addr[6] | out | IOT29[B] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
B2/0 | O_ddr_addr[13] | out | IOT31[A] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
A2/0 | O_ddr_addr[9] | out | IOT31[B] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
D6/0 | O_ddr_ba[0] | out | IOT33[A] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
C6/0 | O_ddr_addr[7] | out | IOT33[B] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
B3/0 | O_ddr_addr[2] | out | IOT35[A] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
A3/0 | O_ddr_addr[0] | out | IOT35[B] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
B4/0 | O_ddr_addr[4] | out | IOT37[A] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
A4/0 | O_ddr_ba[1] | out | IOT37[B] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
C5/0 | O_ddr_cke | out | IOT39[A] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
A5/0 | O_ddr_addr[12] | out | IOT39[B] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
F7/0 | O_ddr_odt | out | IOT41[A] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
E6/0 | O_ddr_addr[10] | out | IOT41[B] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
B6/0 | O_ddr_addr[11] | out | IOT43[A] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
A6/0 | O_ddr_addr[1] | out | IOT43[B] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
E7/0 | O_ddr_cs_n | out | IOT45[A] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
E8/0 | O_ddr_we_n | out | IOT45[B] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
C7/0 | O_ddr_addr[3] | out | IOT48[A] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
A7/0 | O_ddr_reset_n | out | IOT48[B] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
D8/0 | O_ddr_ba[2] | out | IOT50[A] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
C8/0 | O_ddr_addr[5] | out | IOT50[B] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
G8/0 | O_ddr_ras_n | out | IOT52[A] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
F8/0 | O_ddr_cas_n | out | IOT52[B] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
B8/0 | - | in | IOT54[A] | LVCMOS15 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
A8/0 | - | in | IOT54[B] | LVCMOS15 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
D9/0 | O_ddr_clk | out | IOT56[A] | SSTL15D_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
C9/0 | O_ddr_clk_n | out | IOT56[B] | SSTL15D_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
B9/0 | led[2] | out | IOT58[A] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
A9/0 | - | in | IOT58[B] | LVCMOS15 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
D11/1 | IO_ddr_dqs[0] | io | IOT61[A] | SSTL15D_I | 8 | NONE | OFF | NONE | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
C11/1 | IO_ddr_dqs_n[0] | io | IOT61[B] | SSTL15D_I | 8 | NONE | OFF | NONE | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
C10/1 | IO_ddr_dq[5] | io | IOT63[A] | SSTL15_I | 8 | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
A10/1 | IO_ddr_dq[7] | io | IOT63[B] | SSTL15_I | 8 | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
G9/1 | IO_ddr_dq[2] | io | IOT66[A] | SSTL15_I | 8 | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
F9/1 | O_ddr_dqm[0] | out | IOT66[B] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
B11/1 | IO_ddr_dq[1] | io | IOT68[A] | SSTL15_I | 8 | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
A11/1 | IO_ddr_dq[4] | io | IOT68[B] | SSTL15_I | 8 | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
G11/1 | IO_ddr_dq[3] | io | IOT70[A] | SSTL15_I | 8 | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
F10/1 | IO_ddr_dq[6] | io | IOT70[B] | SSTL15_I | 8 | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
A12/1 | IO_ddr_dq[0] | io | IOT72[B] | SSTL15_I | 8 | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
F11/1 | IO_ddr_dq[11] | io | IOT74[A] | SSTL15_I | 8 | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
E11/1 | IO_ddr_dq[10] | io | IOT74[B] | SSTL15_I | 8 | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
D12/1 | IO_ddr_dq[13] | io | IOT76[A] | SSTL15_I | 8 | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
C12/1 | IO_ddr_dq[12] | io | IOT76[B] | SSTL15_I | 8 | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
C13/1 | IO_ddr_dq[8] | io | IOT78[A] | SSTL15_I | 8 | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
A13/1 | IO_ddr_dq[9] | io | IOT78[B] | SSTL15_I | 8 | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
F12/1 | IO_ddr_dqs[1] | io | IOT80[A] | SSTL15D_I | 8 | NONE | OFF | NONE | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
E12/1 | IO_ddr_dqs_n[1] | io | IOT80[B] | SSTL15D_I | 8 | NONE | OFF | NONE | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
B14/1 | IO_ddr_dq[14] | io | IOT83[A] | SSTL15_I | 8 | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
A14/1 | IO_ddr_dq[15] | io | IOT83[B] | SSTL15_I | 8 | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
F13/1 | O_ddr_dqm[1] | out | IOT85[A] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
E13/1 | - | in | IOT85[B] | LVCMOS15 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
C15/1 | - | in | IOT87[A] | LVCMOS15 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
A15/1 | key_in0 | in | IOT87[B] | SSTL15_I | OFF | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
D14/1 | led[0] | out | IOT89[A] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
C14/1 | led[1] | out | IOT89[B] | SSTL15_I | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
B16/1 | reset_n | in | IOT91[A] | SSTL15_I | OFF | NONE | OFF | NONE | OFF | INTERNAL | OFF | OFF | 1.5 | MEDIUM
A16/1 | - | in | IOT91[B] | LVCMOS15 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 1.5 | MEDIUM
V2/5 | - | in | IOB1[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
T4/5 | - | in | IOB2[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
N5/5 | - | in | IOB4[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
P6/5 | - | in | IOB4[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
R7/5 | hdmi_dat_p[0] | out | IOB6[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
T7/5 | hdmi_dat_n[0] | out | IOB6[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
R3/5 | - | in | IOB8[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
T3/5 | - | in | IOB8[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
U5/5 | - | in | IOB10[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
V5/5 | - | in | IOB10[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
R5/5 | hdmi_dat_p[2] | out | IOB12[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
T5/5 | hdmi_dat_n[2] | out | IOB12[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
N6/5 | - | in | IOB14[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
P7/5 | - | in | IOB14[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
T6/5 | hdmi_dat_p[1] | out | IOB16[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
V6/5 | hdmi_dat_n[1] | out | IOB16[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
P8/5 | - | in | IOB18[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
U7/5 | - | in | IOB20[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
V7/5 | - | in | IOB20[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
U8/5 | uart_rx | in | IOB22[A] | LVCMOS33 | OFF | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
V8/5 | - | in | IOB22[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
M8/5 | - | in | IOB24[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
N8/5 | - | in | IOB24[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
M10/5 | hdmi_clk_p | out | IOB26[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
N9/5 | hdmi_clk_n | out | IOB26[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
T9/4 | clk50m | in | IOB29[A] | LVCMOS33 | OFF | NONE | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
V9/4 | - | in | IOB29[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
R8/4 | - | in | IOB31[A] | LVCMOS33 | 8 | NONE | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
T8/4 | - | in | IOB31[B] | LVCMOS33 | 8 | NONE | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
U10/4 | - | in | IOB33[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
V10/4 | - | in | IOB33[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
R10/4 | - | in | IOB35[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
T10/4 | - | in | IOB35[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
U3/4 | - | in | IOB37[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
V3/4 | - | in | IOB37[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
U11/4 | - | in | IOB39[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
V11/4 | - | in | IOB39[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
N10/4 | - | in | IOB41[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
P11/4 | - | in | IOB41[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
T12/4 | - | in | IOB43[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
V12/4 | - | in | IOB43[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
R11/4 | - | in | IOB45[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
T11/4 | - | in | IOB45[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
M11/4 | - | in | IOB48[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
N11/4 | - | in | IOB48[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
U13/4 | - | in | IOB50[A] | LVCMOS33 | 8 | NONE | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
V13/4 | - | in | IOB50[B] | LVCMOS33 | 8 | NONE | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
N12/4 | - | in | IOB52[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
P12/4 | - | in | IOB52[B] | LVCMOS33 | 8 | NONE | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
T14/4 | - | in | IOB54[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
V14/4 | - | in | IOB54[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
U15/4 | - | in | IOB56[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
V15/4 | - | in | IOB56[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
R13/4 | - | in | IOB58[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
T13/4 | - | in | IOB58[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
U16/4 | - | in | IOB60[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
V16/4 | - | in | IOB60[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
R15/4 | - | in | IOB62[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
T15/4 | - | in | IOB62[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
V17/4 | - | in | IOB64[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
P15/3 | - | in | IOB65[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
P16/3 | - | in | IOB65[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
L14/3 | TFT_rgb[8] | out | IOB67[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
M13/3 | TFT_rgb[7] | out | IOB67[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
M14/3 | TFT_clk | out | IOB69[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
N14/3 | TFT_rgb[4] | out | IOB69[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
U17/3 | TFT_pwm | out | IOB71[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
U18/3 | TFT_de | out | IOB71[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
T17/3 | TFT_vs | out | IOB73[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
T18/3 | TFT_hs | out | IOB73[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
N15/3 | TFT_rgb[3] | out | IOB75[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
N16/3 | TFT_rgb[2] | out | IOB75[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
P17/3 | - | in | IOB77[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
P18/3 | - | in | IOB77[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
N17/3 | - | in | IOB79[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
N18/3 | - | in | IOB79[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
M16/3 | TFT_rgb[1] | out | IOB81[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
M18/3 | TFT_rgb[0] | out | IOB81[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
L17/3 | - | in | IOB83[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
L18/3 | - | in | IOB83[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
K17/3 | - | in | IOB85[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
K18/3 | - | in | IOB85[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
J16/3 | TFT_rgb[6] | out | IOB87[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
H17/3 | - | in | IOB89[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
H18/3 | - | in | IOB89[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
L15/3 | TFT_rgb[10] | out | IOB91[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
L16/3 | TFT_rgb[9] | out | IOB91[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
H2/6 | - | in | IOL3[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
H1/6 | - | in | IOL3[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
K4/6 | - | in | IOL5[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
K3/6 | - | in | IOL5[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
J1/6 | - | in | IOL7[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
L4/6 | - | in | IOL9[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
L3/6 | - | in | IOL9[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
K2/6 | - | in | IOL12[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
K1/6 | - | in | IOL12[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
L2/6 | - | in | IOL14[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
L1/6 | - | in | IOL14[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
M3/6 | - | in | IOL16[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
M1/6 | - | in | IOL16[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
N2/6 | - | in | IOL18[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
N1/6 | - | in | IOL18[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
P2/6 | - | in | IOL21[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
P1/6 | - | in | IOL21[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
A17/10 | - | in | IOR1[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
D15/10 | - | in | IOR1[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
B18/10 | - | in | IOR3[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
D16/10 | - | out | IOR3[B] | LVCMOS33 | 8 | UP | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
H12/2 | TFT_rgb[15] | out | IOR5[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
G13/2 | TFT_rgb[14] | out | IOR5[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
F14/2 | uart_rx_flag | out | IOR7[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
G14/2 | uart_data_img[3] | out | IOR7[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
C17/2 | uart_byte_vaild_r0 | out | IOR9[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
C18/2 | image_data_valid_r0 | out | IOR9[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
D17/2 | uart_data_img[4] | out | IOR12[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
D18/2 | uart_data_img[5] | out | IOR12[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
F15/2 | TFT_rgb[13] | out | IOR14[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
F16/2 | TFT_rgb[12] | out | IOR14[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
E16/2 | - | in | IOR16[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
E18/2 | TFT_rgb[11] | out | IOR16[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
H13/2 | uart_data_img[2] | out | IOR18[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
H14/2 | - | in | IOR18[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
F17/2 | uart_data_img[1] | out | IOR20[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
F18/2 | uart_data_img[0] | out | IOR20[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
G16/2 | uart_data_img[6] | out | IOR22[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
G18/2 | uart_data_img[7] | out | IOR22[B] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
H15/2 | TFT_rgb[5] | out | IOR24[A] | LVCMOS33 | 8 | NONE | OFF | OFF | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
J13/2 | - | in | IOR26[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
K14/2 | - | in | IOR26[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
K12/2 | - | in | IOR29[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
K13/2 | - | in | IOR29[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
L12/2 | - | in | IOR31[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
L13/2 | - | in | IOR31[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
K15/2 | - | in | IOR33[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
K16/2 | - | in | IOR33[B] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM
R16/11 | - | in | IOR35[A] | LVCMOS33 | 8 | UP | OFF | ON | OFF | OFF | OFF | OFF | 3.3 | MEDIUM